Just tap water is safe to eat

Gunsan k-water quality test results

( December, 2014 )

Yongdam process water purification treatment process through the scientific safe and clean water

Water Source

【 Youngdam Front view 】

Water Treatment Process

Disinfection Place

Water supply

intake Water  Place

Start Place

Mixed Place

Aggregation Place

Sedimentation Place

Filtration Place

Disinfection Place

Home

Water treatment plant and reservoir inflow

K-water produces a monthly water quality test results in water suitable for drinking     water as the water is received is determined

○ Water sampling date : December 5, 2014

○ Test period : December 6, 2014  ~  December 22, 2014

No.	Test items	water standards	Test results		No.	Test items	water standards	Test results
			Water Plant	Gunsan water				Water Plant	Gunsan water
1	Bacteria	100CFU/㎖Less	0	0	30	1,2dibromo-3-chloropropane	0.003㎎/ℓLess	ND	ND
2	Total Coliforms	ND/100㎖	ND	ND	31	1,4-dioxane	0.05㎎/ℓLess	ND	ND
3	E.coli	ND/100㎖	ND	ND	32	Residual chlorine	4.0㎎/ℓLess	0.77	0.42
4	Pb	0.01㎎/ℓLess	ND	ND	33	Trihalomethanes	0.1㎎/ℓLess	0.018	0.023
5	F	1.5㎎/ℓLess	ND	ND	34	chloroform	0.08㎎/ℓLess	0.014	0.018
6	As	0.01㎎/ℓLess	ND	ND	35	bromodichloromethane	0.03㎎/ℓLess	0.004	0.005
7	Se	0.01㎎/ℓLess	ND	ND	36	dibromochloromethane	0.1㎎/ℓLess	ND	ND
8	Hg	0.001㎎/ℓLess	ND	ND	37	chloralhydrate	0.03㎎/ℓLess	0.0022	0.0043
9	CN	0.01㎎/ℓLess	ND	ND	38	Dibromoacetonitrile	0.1㎎/ℓLess	ND	ND
10	Cr	0.05㎎/ℓLess	ND	ND	39	Dichloroacetonitrile	0.09㎎/ℓLess	0.0015	0.0023
11	NH3-N	0.5㎎/ℓLess	ND	ND	40	Trichloroacetonitrile	0.004㎎/ℓLess	ND	ND
12	NO3-N	10㎎/ℓLess	1.4	1.4	41	Haloaceticacid	0.1㎎/ℓLess	0.019	0.022
13	Cd	0.005㎎/ℓLess	ND	ND	42	Formaldehyde	0.2㎎/ℓLess	ND	ND
14	B	1.0㎎/ℓLess	ND	ND	43	Hardness	300㎎/ℓLess	38	36
15	Phenol	0.005㎎/ℓLess	ND	ND	44	Donsumption of ptas sium permanganate	10㎎/ℓLess	1.0	1.1
16	Diazinon	0.02㎎/ℓLess	ND	ND	45	Smell	only the raw smell of disinfection	None	None
17	Parathion	0.06㎎/ℓLess	ND	ND	46	Taste	only the raw taste of disinfection	None	None
18	Fenitrothion	0.04㎎/ℓLess	ND	ND	47	Cu	1㎎/ℓLess	ND	ND
19	Carbaryl	0.07㎎/ℓLess	ND	ND	48	Color	5 Less	ND	ND
20	1.1.1-Trichloroethane	0.1㎎/ℓLess	ND	ND	49	ABS	0.5㎎/ℓLess	ND	ND
21	Tertachloroethylene	0.01㎎/ℓLess	ND	ND	50	PH	5.8 ~ 8.5	7.2	7.1
22	Trichloroethylene	0.03㎎/ℓLess	ND	ND	51	Zn	3㎎/ℓLess	ND	0.004
23	Dichloromethane	0.02㎎/ℓLess	ND	ND	52	Cl-	250㎎/ℓLess	10.8	10.1
24	Benzene	0.01㎎/ℓLess	ND	ND	53	Residue on evaporation	500㎎/ℓLess	55	54
25	Toluene	0.7㎎/ℓLess	ND	ND	54	Fe	0.3㎎/ℓLess	ND	ND
26	Ethylbenzene	0.3㎎/ℓLess	ND	ND	55	Mn	0.05㎎/ℓLess	ND	ND
27	Xylene	0.5㎎/ℓLess	ND	ND	56	Turbidity	0.5NTULess	0.05	0.05
28	1.1-Dichloroethylene	0.03㎎/ℓLess	ND	ND	57	SO42-	200㎎/ℓLess	7	6
29	Tetrchlorocarbon	0.002㎎/ℓLess	ND	ND	58	Al	0.2㎎/ℓLess	ND	ND
Test results			Suitable	Suitable	Test results			Suitable	Suitable

K-water courses by reservoir(Water test results from participating in Gunsan volunteers society women)

Regional water quality test results for 16 sites suitable for drinking

○ Water sampling date : November 17, 2014 ~ November 18, 2014

○ Test period : November 17, 2014 ~ December 2, 2014

▶ Naun reservoir

Division	P H (5.8~3.5)	Residual chlorine (4.0mg/ℓLess)	Turbidity (0.5NTU Less)	Bacteria (100CFU/mℓLess)	Total Coliforms (NE/100mℓ)	E.coli (ND/100mℓ Less)	NH3-N (0.5mg/ℓ Less)	Fe (0.3mg/ℓ Less)	Cu (1mg/ℓ Less)	Zn (3mg/ℓ Less)	Trihalomethanes(0.1mg/ℓLess)
Average	6.6	0.06	0.11	0	ND	ND	ND	0.03	ND	0.001	0.059
Max	6.6	0.11	0.21	0	ND	ND	ND	0.11	ND	0.002	0.061

▶ Kunbong reservoir

Division	P H (5.8~3.5)	Residual chlorine (4.0mg/ℓLess)	Turbidity (0.5NTU Less)	Bacteria (100CFU/mℓ Less)	Total Coliforms (NE/100mℓ)	E.coli (ND/100mℓ Less)	NH3-N (0.5mg/ℓ Less)	Fe (0.3mg/ℓ Less)	Cu (1mg/ℓ Less)	Zn (3mg/ℓ Less)	Trihalomethanes(0.1mg/ℓLess)
Average	6.5	0.02	0.09	0	ND	ND	ND	ND	ND	0.003	0.048
Max	6.6	0.07	0.11	0	ND	ND	ND	ND	ND	0.005	0.058

▶ Daeya reservoir

Division	P H (5.8~3.5)	Residual chlorine (4.0mg/ℓLess)	Turbidity (0.5NTU Less)	Bacteria (100CFU/mℓLess)	Total Coliforms (NE/100mℓ)	E.coli (ND/100mℓ Less)	NH3-N (0.5mg/ℓ Less)	Fe (0.3mg/ℓLess)	Cu (1mg/ℓLess)	Zn (3mg/ℓLess)	Trihalomethanes(0.1mg/ℓLess)
Average	6.5	0.07	0.09	0	ND	ND	ND	ND	ND	ND	0.060
Max	6.6	0.12	0.13	0	ND	ND	0.01	ND	ND	ND	0.062

▶ Ohsikdo reservoir

Division	P H (5.8~3.5)	Residual chlorine (4.0mg/ℓLess)	Turbidity (0.5NTU Less)	Bacteria (100CFU/mℓ Less)	Total Coliforms (NE/100mℓ)	E.coli (ND/100mℓ Less)	NH3-N (0.5mg/ℓ Less)	Fe (0.3mg/ℓLess)	Cu (1mg/ℓ Less)	Zn (3mg/ℓ Less)	Trihalomethanes(0.1mg/ℓ Less)
Average	6.7	0.09	0.07	0	ND	ND	0.025	ND	0.013	ND	0.018
Max	6.8	0.14	0.09	0	ND	ND	0.01	ND	ND	ND	0.019

Faucet(Water test results from participating in Gunsan, Korea Women Consumers Union)

Every month 40 locations in tap water safety test results

○ Water sampling test : December 8, 2014 ~ December 10, 2014

○ Test period : December 8, 2014. ~ December 22, 2014

▶ Faucet

Bacteria (100CFU/㎖Less)		Totalcoliforms (ND/100㎖)		E.coli (ND/100㎖)		Residual chlorine (4.0mg/ℓLess)
Average	Max	Average	Max	Average	Max	Average	Max
0	0	ND	ND	ND	ND	0.31	0.47

▶ After passing through a water tank faucet

Bacteria (100CFU/㎖Less)		Totalcoliforms (ND/100㎖)		E.coli (ND/100㎖)		Residual chlorine (4.0mg/ℓLess)
Average	Max	Average	Max	Average	Max	Average	Max
0	0	ND	ND	ND	ND	0.23	0.35

▶ The end of the faucet

구 분	Bacteria (100CFU/mℓLess)	Totalcoliforms (ND/100mL)	E.coli (ND/100mL)	Residual chlorine (4.0 mg/ℓLess)	Fe (0.3 mg/ℓLess)	Cu (1 mg/ℓLess)	Zn (3 mg/ℓLess)	Mn (0.3 mg/ℓLess)	NH3-N (0.5 mg/ℓLess)	Cl- (250mg/ℓLess)
Average value	0	ND	ND	0.42	ND	ND	0.001	ND	ND	11
Maximum value	0	ND	ND	0.46	ND	ND	0.004	ND	ND	13

Contact water quality

♣ Counter complaints : Gunsan city water service section

♣ Complaints Phone : No area code 120times

☎ Adminstration 454-5352 Charge 454-5362

Water Mangement 454-5382 Water sector 454-5392, 5402, 5422

Monthly water quality test results reveal the homepage